Unit 109: Plastering and interior systems

# Worksheet 24: General knowledge questions (learner)

1. Cutting out the joints in brickwork is known as?
2. Which plaster is compatible with smooth dense background?
3. What does PVA stand for?
4. How is a simple test carried out for checking for suction on a background?
5. If you have flaking paint on a wall to be re-plastered what must you do?
6. What must you do to small cracks prior to re-skimming a wall?
7. Why is it important to have an even suction in the background before applying plaster?
8. Dust left on the background before plastering can cause what problem?
9. What materials are mixed to make a spatter dash slurry?
10. Which type of hammer is used to form a key?