Unit 109: Plastering and interior systems

# Worksheet 34: Specification (tutor)

This is a group activity.

Design a typical specification for the internal plastering of a new two-bedroom detached house, using solid plaster, plasterboard and accessories.

Write your answer below.

Timber joists and studwork to be fixed with 12.5mm thick 2.400mm x 1.200mm plasterboard using dry wall fixings and finished using gypsum board or multi-finish plaster. External angles to be reinforced with thin coat beads and all plasterboard joints to be reinforced with self-adhesive scrim.

All solid block backgrounds to be fixed with standard angle beads to all openings, windows, doors and returns.

Block backgrounds to be plastered using a two-coat gypsum-based undercoat backing plaster minimum 10mm thick and finished with a 2–3mm multi-finish plaster to industry standards.