Unit 109: Plastering and interior systems

# Worksheet 52: Plastering process questions (learner)

1. Briefly describe where three-coat work would be used.
2. How would you overcome problems such as timber wall plates and concrete lintels?
3. Where and how would a ‘pricking up’ coat be applied?
4. When using cement/sand-based mixes, why is it important to use a weaker mix when adding more coats?
5. When applying floating coats to window walls with beads, state the preparation to avoid the finishing plaster becoming proud along the bead.
6. Name three methods that can be used to apply and form a floating coat.
7. How is a floating coat keyed and prepared for the application of finish?
8. How is a completed two-coat float and finish system on a solid background checked for alignment?
9. What is meant by cutting back at beads?
10. Why is it necessary to scrape down a floating coat prior to applying the finish?