Unit 110: Decorative finishing and industrial painting occupations

# Multiple choice questions (learner)

1. Which is NOT a role of a painter and decorator?
2. Health and safety
3. Planning
4. Spraying cars
5. Preparation
6. Which of the following would be considered industrial work?
7. An electricity pylon
8. A garden wall
9. A school classroom
10. A hairdressing salon
11. What is the name of the horizontal rail close to the handle on a six--panel door?
12. Lock rail
13. Style
14. Muntin
15. Intermediate rail
16. The area of wall above the picture rail is known as:
17. The frieze
18. The dado
19. Cornice
20. Alcove
21. Which of the following colours is the correct colour for a pipe containing acids or alkalis?
22. Brown
23. Violet
24. Red
25. Blue
26. Which paint additive would help a in a situation where sanitation was an important factor?
27. White spirit
28. Biocide
29. Sugar soap
30. Pesticide
31. Of the following abbreviations, which is an Act of Parliament?
32. HASAWA
33. COSHH
34. PUWER
35. RIDDOR
36. In order to be able to carry out a COSHH assessment a person must be:
37. Confident
38. Incompetent
39. A non-employee of the company
40. Competent
41. What is placed on an employer so they MUST carry out risk assessments in the workplace?
42. Pressure from the HSE
43. Duties from the HASAWA
44. A high court writ
45. Regulations
46. What is the correct category for a product with a VOC content between 25 and 50%?
47. Medium
48. Very high
49. High
50. Minimal
51. What would the brush pictured below normally be used for?
52. Applying wallpaper paste
53. Washing down
54. Removing dust from a surface
55. Applying oil-based primer
56. Which tool would be the best choice for removing paint from a moulding on a skirting board?
57. 25mm filling knife
58. Triangular shave hook
59. Combination shave hook
60. Skeleton gun
61. Name the type of paint that is better suited to brushes with synthetic filament fillings.
62. Water-based gloss
63. Oil-based gloss
64. Low VOC undercoat
65. High VOC undercoat
66. Which type of roller sleeve would be used to apply gloss to a flush door?
67. Medium pile sheepskin
68. Extra long woven pile
69. Medium pile polyester
70. Short pile mohair
71. Which is a coarse grade of aluminium oxide paper?
72. 90
73. 60
74. 50
75. 110
76. Of the fillers below, which could be used on an exterior metal door?
77. Exterior masonry filler
78. Two pack filler
79. Fine surface filler
80. Exterior powder filler
81. Which of the following is true regarding water-based eggshell paint?
82. It is quick drying
83. Brush marks flow out easily
84. It has a strong odour
85. It has a deep glossy sheen
86. Which of the coatings below is a transparent coating for wood?
87. Emulsion
88. Gloss
89. Varnish
90. primer
91. You have to protect a polished wooden floor in a busy entrance, what would be the safest type of protection?
92. Cotton dust sheet
93. Rubber-backed cotton dust sheet
94. Heavy duty tarpaulin
95. Masking tape
96. Easily torn, not durable, needs taping down, translucent, are all characteristics of which type of masking material?
97. Lightweight polythene sheet
98. Tarpaulin
99. Cotton dust sheets
100. Brown masking paper
101. Which of the following is the correct colour and voltage for electrical equipment used on site?
102. Red 110 volts
103. Blue 240 volts
104. Yellow 240 volts
105. Yellow 110 volts
106. The first coat of paint on bare wood or metal is called:
107. Undercoat
108. Primer
109. Eggshell
110. Gloss