Unit 111: Roofing occupations

# Worksheet 5: Plain tile – establishing first course and eaves batten position (learner)

Finding the first fix point: fill in the gaps below.

1. Turn the roof tile over and measure from the underside of the to the tail. Repeat this for the tile and note both measurements.
2. Take your and extend the end of it over the (or halfway into the gutter, whichever is smaller).
3. the points at both ends of the roof and lines between them.
4. Fix the battens with the top edge to the (just a few nails, not driven).
5. The top edges of the battens are the first fixed points for the double course at eaves. Try a tile and an under-eaves tile at each end to make sure that they overhang and that the are in before continuing.