Unit 116: Carry out wall and floor tiling tasks

# Worksheet 43: Wall tiling panel with cut tiles (learner)

You can try this task many times to allow completion to a satisfactory standard. You should work individually to complete the task. Centres can amend the dimensions of the task to suit different abilities and workstation sizes. The contrasting tiles are added so you can work to a specification; colours can be varied to meet the centre’s stock.

|  |
| --- |
|  |
| **Key points**   * Learner has responsibility to ensure backgrounds are suitably prepared * Set out task using skills learned * Recommend: use of fixing batten/rule to support wall tiles during task * Apply adhesive to allow 90% coverage on tiles * Gauge tiles to meet overall dimensions (under/over-sized tiles) * Recommend: 150mm square wall tiles * Recommend: 2mm spacers * Recommend: cut tiles dimension is 75mm (half tiles) * Excess adhesive and grout marks are removed from task boundaries * All grout lines to be tooled * PPE must be worn as appropriate to task * Work area to be kept clean and tidy during activity * Learner to ‘self-score’ and evaluate their work prior to marking by tutor |
| Learners should have overall responsibility for using and maintaining tools and equipment used |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Learner’s name:** |  | **Points (Learning outcome 5.1)** | | | |
| **The learner has:** | **Learning outcome** | **Tutor’s score** | | | **Learner’s self-score** |
| **1** | **2** | **3** |
| *selected and used appropriate tools correctly* | **4.1** | tickbox  Met |  |  |  |
| *suitably prepared background* | **4.2** | tickbox  Met |  |  |  |
| *set out wall dimension* | **4.3** | tickbox  +/-3mm | tickbox  +/-2mm | tickbox  +/- 1mm |  |
| *installed tiles level (check top + mid-level line)* | **4.4** | tickbox  +/-3mm | tickbox  +/-2mm | tickbox  +/-1mm |  |
| *installed tiles plumb (check both ends)* | **4.4** | tickbox  +/-3mm | tickbox  +/-2mm | tickbox  +/-1mm |  |
| *installed tiles to alignment*  *(diagonal face plane) x2* | **4.4** | tickbox  +/-3mm | tickbox  +/-2mm | tickbox  +/-1mm |  |
| *equal joint sizes: +/-1mm*  *(spacer size: 2mm)* | **4.4** | tickbox  ≤ 3 | tickbox  ≥ 2 | tickbox  None |  |
| *produced a flat and specific appearance (no lipping, contrasting tiles suitably positioned)* | **4.4** | tickbox  ≤ 3 | tickbox  ≥ 2 | tickbox  None |  |
| *appropriately applied adhesive* | **4.5** | tickbox  Met |  |  |  |
| *used grout effectively (full coverage, no pin holes, clean appearance-no grout stains, polished)* | **4.6** | tickbox  ≤ 3 | tickbox  ≥ 2 | tickbox  None |  |
| *worn PPE as required with no warnings* | **4.7** | tickbox  ≤ 2 | tickbox  ≥ 1 | tickbox  None |  |
| *kept a clean and tidy work area with no warnings* | **4.7** | tickbox  ≤ 2 | tickbox  ≥ 1 | tickbox  None |  |
| Sub-totals | | /12 | /18 | /27 | /30 |
| Overall total | | /30 | | |  |
| Learner’s evaluation (Learning outcome 5.2) | | | | | |
| Tutor’s comments | | | | | |
| Marked by: …………………………………………. Date completed: ……………………… | | | | | |