Unit 116: Carry out wall and floor tiling tasks

# Worksheet 46: Wall tiling – column with trim (learner)

You can try this task many times to allow completion to a satisfactory standard. It is recommended that you work individually to complete the task. Centres can amend the dimensions of the task to suit different abilities and workstation sizes. You should receive dimensions before starting the task. Centres are advised to silicone the inner angle against the column.

|  |
| --- |
|  |
| **Key points**   * Learner has responsibility to ensure backgrounds are suitably prepared * Set out task using skills learned * Recommend: use of fixing batten/rule to support wall tiles during task * Apply adhesive to allow 90% coverage on tiles * Gauge tiles to meet overall dimensions (under/over-sized tiles) * Recommend: 150mm square wall tiles * Recommend: 2mm spacers * Recommend: column-cut tiles dimension is 75mm (half tiles) * Silicone inner angle against column * Trim is fixed to both sides of the column * Excess adhesive and grout marks are removed from task boundaries * All grout lines to be tooled * PPE must be worn as appropriate to task * Work area to be kept clean and tidy during activity * Learner to ‘self-score’ and evaluate their work prior to marking by tutor |
| Learners should have overall for using and maintaining tools and equipment used |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Learner’s name:** |  | **Points (Learning outcome 5.1)** | | | |
| **The learner has:** | **Learning outcome** | **Tutor’s score** | | | **Learner’s self-score** |
| **1** | **2** | **3** |
| *selected and used appropriate tools correctly* | **4.1** | tickbox  Met |  |  |  |
| *suitably prepared background* | **4.2** | tickbox  Met |  |  |  |
| *set out wall to given dimension* | **4.3** | tickbox  +/-3mm | tickbox  +/-2mm | tickbox  +/- 1mm |  |
| *installed tiles level (check top)* | **4.4** | tickbox  +/-3mm | tickbox  +/-2mm | tickbox  +/-1mm |  |
| *installed tiles plumb (check both sides of column)* | **4.4** | tickbox  +/-3mm | tickbox  +/-2mm | tickbox  +/-1mm |  |
| *equal joint sizes: +/-1mm*  *(spacer size: 2mm)* | **4.4** | tickbox  ≤ 3mm | tickbox  ≥ 2mm | tickbox  None |  |
| *Fixed trim plumb and straight* | **4.4** | tickbox  ≤ 3mm | tickbox  ≥ 2mm | tickbox  None |  |
| *produced a flat and specific appearance (no lipping, contrasting tiles suitably positioned)* | **4.4** | tickbox  ≤ 3 | tickbox  ≥ 2 | tickbox  None |  |
| *appropriately applied adhesive* | **4.5** | tickbox  Met |  |  |  |
| *used grout effectively (full coverage, no pin holes, clean appearance-no grout stains, polished)* | **4.6** | tickbox  ≤ 3 | tickbox  ≥ 2 | tickbox  None |  |
| *used silicone effectively (full coverage, no pin holes, clean appearance-smudges)* | **4.6** | tickbox  ≤ 3 | tickbox  ≥ 2 | tickbox  None |  |
| *worn PPE as required with no warnings* | **4.7** | tickbox  ≤ 2 | tickbox  ≥ 1 | tickbox  None |  |
| *kept a clean and tidy work area with no warnings* | **4.7** | tickbox  ≤ 2 | tickbox  ≥ 1 | tickbox  None |  |
| Sub-totals | | /13 | /20 | /30 | /33 |
| Overall total | | /33 | | |  |
| Learner’s evaluation (Learning outcome 5.2) | | | | | |
| Tutor’s comments | | | | | |
| Marked by: …………………………………………. Date completed: ……………………… | | | | | |