Unit 116: Carry out wall and floor tiling tasks

# Worksheet 49: Floor tiling panel with column (tutor)

You can try this task many times to allow completion to a satisfactory standard. It is recommended that you work individually to complete the task. Centres can amend the dimensions of the task to suit different abilities and workstation sizes, although the column dimensions must be larger than the tiles used. Column to be sited mid-way between two tiles.

This task is to be used in conjunction with Worksheet 47.

|  |
| --- |
|  |
| **Key points**   * Learner has responsibility to ensure backgrounds are suitably prepared * Set out task using skills learned * Apply adhesive to allow 90% coverage on tiles * Gauge tiles to meet overall dimensions (under/over-sized tiles) * Recommend: minimum 200mm square floor tiles * Recommend: 5mm spacers * Excess adhesive and grout marks are removed from task boundaries * All grout lines to be tooled * PPE must be worn as appropriate to task * Work area to be kept clean and tidy during activity * Learner to ‘self-score’ and evaluate their work prior to marking by deliverer |
| Learners should have overall responsibility for using and maintaining tools and equipment used |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Learner’s name:** | | **Points (Learning outcome 5.1)** | | | |
| **The learner has:** | **Learning outcome** | **Tutor’s score** | | | **Learner’s self-score** |
| **1** | **2** | **3** |
| *selected and used appropriate tools correctly* | **4.1** | tickbox  Met |  |  |  |
| *suitably prepared background* | **4.2** | tickbox  Met |  |  |  |
| *set out floor dimension* | **4.3** | tickbox  +/-3mm | tickbox  +/-2mm | tickbox  +/- 1mm |  |
| *installed tiles level (check length and width)* | **4.4** | tickbox  +/-3mm | tickbox  +/-2mm | tickbox  +/-1mm |  |
| *cut tiles accurately around column (check angle and gap)* | **4.4** | tickbox  +/- 3mm | tickbox  +/-2mm | tickbox  +/-1mm |  |
| *installed tiles to alignment (straight edges) x2* | **4.4** | tickbox  +/-3mm | tickbox  +/-2mm | tickbox  +/-1mm |  |
| *installed tiles to alignment*  *(diagonal face plane) x2* | **4.4** | tickbox  +/-3mm | tickbox  +/-2mm | tickbox  +/-1mm |  |
| *equal joint sizes: +/-1mm*  *(spacer size: 2mm)* | **4.4** | tickbox  ≤ 3 | tickbox  ≥ 2 | tickbox  None |  |
| *produced a flat appearance (no lipping)* | **4.4** | tickbox  ≤ 3 | tickbox  ≥ 2 | tickbox  None |  |
| *appropriately applied adhesive* | **4.5** | tickbox  Met |  |  |  |
| *used grout effectively (full coverage, no pin holes, clean appearance-no grout stains, polished)* | **4.6** | tickbox  ≤ 3 | tickbox  ≥ 2 | tickbox  None |  |
| *worn PPE as required with no warnings* | **4.7** | tickbox  ≤ 2 | tickbox  ≥ 1 | tickbox  None |  |
| *kept a clean and tidy work area with no warnings* | **4.7** | tickbox  ≤ 2 | tickbox  ≥ 1 | tickbox  None |  |
| Sub-totals | | /13 | /20 | /30 |  |
| Overall total | | /33 | | | /33 |
| Learner’s evaluation (Learning outcome 5.2) | | | | | |
| Tutor’s comments | | | | | |
| Marked by: …………………………………………. Date completed: ……………………… | | | | | |