Unit 103: Introduction to the built environment life cycle

# Worksheet 4: Designing waste out of projects (learner)

1. What is the next commercially available length of timber after 3.6m?
2. 3.7m
3. 3.8m
4. 3.9m
5. 4.0m
6. FIFO is used when working with what type of materials?
7. Combustible
8. Recyclable
9. Perishable
10. Durable
11. What gas is given off if plasterboard is added to landfill with organic materials?
12. Hydrogen sulphide
13. Nitrogen monoxide
14. Hydrogen cyanide
15. Nitrogen dioxide
16. What does SWMP stand for?
17. Small works monitoring programme
18. Site waste monitoring programme
19. Small works management plan
20. Site waste management plan
21. What is the main purpose of having designated skips on site?
22. To monitor the amount of waste leaving the site
23. To promote a professional corporate image
24. To allow for greater recycling of materials
25. To reduce the amount of landfill taxes paid