Unit 105: Protecting health, safety and the environment when working in the construction and built environment sector

# Multiple choice questions (tutor)

1. Which of the following should have a toe board fitted?
2. Trestle scaffold.
3. Mobile scaffold.
4. Moving escalator.
5. Conveyor belt.
6. On a construction site a safety helmet must be worn by everyone except where?
7. A meeting held in a site hut.
8. Attendance on site is for less than half an hour.
9. The building work is not over 10m high.
10. When guard rails and toe boards are fitted to scaffolding.
11. In relation to electrical safety on site, which **one** of the following four statements is true?
12. Only use 410 Volts.
13. Always carry a portable electric tool by its cable.
14. It is not important if lights are not kept clean.
15. Check for all current PAT labels.
16. When erecting ladders which of the following is **not** correct?
17. The ladder should be placed on firm level ground.
18. The angle of the ladder should be 3 up to 1 out.
19. The ladder must extend by at least 1m or 5 rungs above the landing place.
20. All ladders should be examined on a regular basis. The test results should be recorded.
21. All the following are important considerations before lifting a load **except:**
22. getting help if the load is too heavy.
23. checking that doors are opened if you must carry the load through them.
24. making trial lifts on similar loads.
25. checking the load for any sharp edges.
26. The RIDDOR Act requires your company to inform the enforcing authority without delay of the following circumstances **except**:
27. any major injuries to employees.
28. any fatal injuries.
29. the overturning of a crane.
30. an accident at home.
31. Which of the following should have a handrail fitted?
32. Trestle scaffold.
33. Mobile scaffold.
34. Moving escalator.
35. Conveyor belt.
36. On a construction site, safety boots must be worn by everyone except where?
37. Changing facilities and drying rooms
38. Attendance on site is for less than half an hour.
39. The building work is not over 10m high.
40. When guard rails and toe boards are fitted to scaffolding.
41. In relation to electrical safety on site which **one** of the following four statements is true?
42. Only use 410 Volts.
43. Always carry a portable electric tool by its cable.
44. It is not important if lights are not kept clean.
45. Check for loose wires.
46. When erecting ladders which of the following is **not** correct?
47. The ladder should be placed on firm level ground.
48. The ladder can be painted.
49. The ladder must extend by at least 1m or 5 rungs above the landing place.
50. All ladders should be examined on a regular basis. The test results should be recorded.
51. All the following are important considerations before lifting a load **except:**
52. getting help if the load is too heavy.
53. you can lift a load as heavy as you can.
54. making trial lifts on similar loads.
55. checking the load for any sharp edges.
56. The RIDDOR Act requires your company to inform the enforcing authority without delay of the following circumstances **except:**
57. any major injuries to employees.
58. any fatal injuries.
59. the overturning of a crane.
60. an accident at home.
61. What colour fire extinguisher is suitable for a wood fire?
62. Blue
63. Black
64. Red
65. Green
66. What is the most suitable scaffold platform to use to access a high building?
67. Hop up
68. Podium
69. Trestles
70. Mobile tower
71. What does HSE stand for?
72. Health and Safety Elite
73. Hazard and safety employee
74. Health and Safety Executive
75. Hazard and Substance Emissions
76. Who would you report an accident to on site?
77. Groundworker
78. Technician
79. Supervisor
80. Painter
81. Where should harmful chemicals be disposed of on site?
82. In a works vehicle
83. In a designated skip
84. In a trench
85. In a black container
86. What colour safety sign is a prohibition sign?
87. Green and white
88. Red and black
89. Red and yellow
90. Blue and white
91. Which of the following would not be part of a first aid kit?
92. Plasters
93. Bandages
94. Scissors
95. Wipes
96. What is a mandatory welfare requirement on site?
97. Bike huts
98. Food outlets
99. Toilets
100. Car parks