Unit 105: Protecting health, safety and the environment when working in the construction and built environment sector

# Worksheet 22: Site services (tutor)

Answer the following questions about workplace safety.

1. Which one of the following is a fire hazard if stored incorrectly?
2. LPG bottles.
3. Steel lintels.
4. PVA adhesives.
5. Drainage pipes.
6. Which one of the following is a typical risk associated with the incorrect storage of concrete drain pipes?
7. Electrocution.
8. Crushing.
9. Dermatitis.
10. Suffocation.
11. What is the hazard associated with damaged electrical services on site?
12. Fire.
13. Corrosion.
14. Heat loss.
15. Contamination.

1. What is the hazard associated with damaged gas services on site?
2. Heat loss.
3. Corrosion.
4. Fire.
5. Contamination.

1. Which one of the following is classed as a major hazard associated with services to a building?
2. A damaged phone cable.
3. An exposed sewer.
4. An exposed gas main.
5. A damaged electrical supply.
6. Which one of the following is a typical hazard associated with services?
7. Exposed sewer.
8. Disused gas supply.
9. Worn electric cables.
10. Exposed phone cable.