Unit 108: Wood occupations

# Worksheet 26: First and second fix activities (tutor)

You are required to select two correct answers for each of the following multi-choice questions

1. Which items of PPE should be worn when using a router?
2. Lanyard.
3. Respirator.
4. Dust mask.
5. Rigger gloves.
6. Ear defenders.
7. What is likely to happen if the riving knife is removed from a circular saw?
8. The saw will kick back.
9. The saw will bind in the cut.
10. The cut will be easier to start.
11. The extractor will clear chips faster.
12. The cut may meander from straight.
13. Which joints are normally used to make a wooden window frame?
14. Butt.
15. Comb.
16. Half lap.
17. Dovetail joint.
18. Mortice and tenon.

1. Which joints are used when fitting skirting?
2. Mitre.
3. Scarf
4. Comb.
5. Scribe.
6. Housing
7. Which methods are used when fitting floor boarding?
8. Leaving 10mm perimeter clearance.
9. Cutting all boards to the same length.
10. Cramping boards tight using sash cramps.
11. Punching all nails below the board surface**.**
12. Positioning all heading joints over the same joist.
13. Which type of joints are normally used when fitting a door lining?
14. Slip dovetail.
15. Stub mortice.
16. Dovetail housing.
17. Stopped housing.
18. Tongued housing.
19. What operations can be carried out using a portable router?
20. Planing.
21. Grooving.
22. Morticing.
23. Moulding.
24. Thicknessing.
25. What operations can be carried out using a power planer?
26. Bevelling.
27. Grooving.
28. Morticing.
29. Tapering.
30. Moulding.
31. What power tools are required when forming an internal corner kitchen worktop joint?
32. Router.
33. Planer.
34. Doweller.
35. Biscuit jointer.
36. Framing nailer.
37. Which are uses of a sliding bevel?
38. Marking out 90° cuts on floor boards.
39. Marking out a pattern common rafter.
40. Marking out treads and risers on a stair string.
41. Marking out curved shapes on plywood sheeting.
42. Marking out mitres on skirting around a bay window.

.