Unit 108: Wood occupations

# Worksheet 3: Trades that work with site carpenters (tutor)

1. List **four** trades who a site carpenter would need to communicate with in the built environment and what information/work they might require/share:

|  |  |
| --- | --- |
| **Trade:** | **Information:** |
| Bricklayer | Datum values, templets for arch centres and curved walls, pegs for setting out, dummy frames for openings |
| Electrician | Where holes/notching is required for cable runs, where noggins are required for steel electrical boxes in stud partitions, where service runs have been positioned |
| Plumber | Where holes/notching is required for cable runs, where noggins are required within stud partitions for plumbing second fixings such as wall hung basins, where service runs have been positioned |
| Plasterer | Fixing positions of gauges, making any templets required, projections of linings from the face of plasterboard |
| Specialist contractors such as ceiling fixers, kitchen fixers, wall and floor tilers | Fixing positions and timings of operations |