Unit 109: Plastering and interior systems

# Worksheet 16: True or false (tutor)

Recap questions: true or false?

1. PVA can be diluted with water.

True

1. Thin coat stop beads are designed for two coat float and finish application

False

1. Plasterboard can be fixed with galvanised nails.

True

1. Beads can be fixed with plaster dabs.

True

1. Reinforced tape is used for plasterboard internal angle.

False

1. Stop beads are used on window returns.

False

1. Dry wall primer is applied over tape and jointed surfaces.

True

1. External jointed surfaces do not require sanding before applying primer.

False

1. Perforated tape is a stronger reinforcement than EML coil.

False

1. Expanded metal also comes in sheets.

True