Unit 109: Plastering and interior systems

# Worksheet 42: True or false (learner)

Read the following statements and state whether they are true or false.

1. Plasterboards can be fixed with foam adhesive.
2. Plasterboard has a gypsum core.
3. Ivory colour coded plasterboard is moisture resistant.
4. Blue colour coded plasterboard has one-hour fire rating.
5. When fixing plasterboard to steel studs the screw must penetrate the stud 10mm.
6. Thermal laminates are used for increasing insulation.
7. Plasterboard can either be tapered or square edge.
8. When fixing plasterboard to both side of a steel stud partition, the boards will need to be staggered at either side for strength.
9. Plasterboards can only be fixed vertically.
10. Standard plasterboard used in wet rooms can perish.