Unit 109: Plastering and interior systems

# Worksheet 45: Producing a traditional hard angle (learner)

1. Arrange these sentences in the correct order of procedures for creating a hard angle using the reverse rule method. Write them in order from 1 to 9.

Position rule, ensuring plumb

Apply material flush with rule to form external angle

Position rule, ensuring plumb

Hold rule to opposite side

Apply material flush to rule

Slide rule away carefully from nib

Slide rule away once material is set and make good

Check for thickness and plumb

Allow material to set