Unit 109: Plastering and interior systems

# Worksheet 48: Checks carried out when fixing beads (learner)

1. Match the following checks with the activities listed below. Write the activity alongside the checks:

**Checks: Activities:**

Correct length

Type of fixing

Before fixing

Checking for straightness

Plumb and level

Correct dimensions

Equal margins

Square

No steps

Cut back

Left clean and sharp

**Activities:**

Accurate dimensions

After keying a floating coat

After applying finishing plaster

Setting out right angles

Reveal, head and soffit

Beads fixed to both returns on a pier

Two beads fixed to a soffit beam

Spirit level

Plaster dab

Straight edge

Apply dabs