Unit 109: Plastering and interior systems

# Worksheet 51: Plaster application (learner)

1. Arrange the following activities in the correct sequence when carrying out plastering work on a new single storey extension. Write out in the correct order below from 1 to 10.

Fit thin coat beads to plasterboard external returns.

Apply setting plaster to walls and partitions.

Fix plasterboards to the ceiling.

Apply self-adhesive scrim to ceiling and perimeter joints.

Apply setting coats to ceilings.

Apply self-adhesive scrim to wall board joints.

Fix EML to wall plates.

Fix plasterboards to studwork.

Apply ﬂoating coat plaster to backgrounds.

Fix standard angle beads to window, door and wall returns.