Unit 109: Plastering and interior systems

# Worksheet 48: Checks carried out when fixing beads (tutor)

1. Match the following checks with the activities listed below. Write the activity alongside the checks:

**Checks: Activities:**

Correct length Accurate dimensions

Type of fixing Plaster dab

Before fixing Apply dabs

Checking for straightness Straight edge

Plumb and level Spirit level

Correct dimensions Two beads fixed to a soffit beam

Equal margins Beads fixed to both returns on a pier

Square Setting out right angles

No steps Reveal, head and soffit

Cut back After keying a floating coat

Left clean and sharp After applying finishing plaster

**Activities:**

Accurate dimensions

After keying a floating coat

After applying finishing plaster

Setting out right angles

Reveal, head and soffit

Beads fixed to both returns on a pier

Two beads fixed to a soffit beam

Spirit level

Plaster dab

Straight edge

Apply dabs