Unit 109: Plastering and interior systems

# Worksheet 51: Plaster application (tutor)

1. Arrange the following activities in the correct sequence when carrying out plastering work on a new single storey extension. Write out in the correct order below from 1 to 10.
2. Fix plasterboards to the ceiling.
3. Fix plasterboards to studwork.
4. Fix standard angle beads to window, door and wall returns.
5. Fix EML to wall plates.
6. Apply ﬂoating coat plaster to backgrounds.
7. Apply self-adhesive scrim to ceiling and perimeter joints.
8. Apply setting coats to ceilings.
9. Fit thin coat beads to plasterboard external returns.
10. Apply self-adhesive scrim to wall board joints.
11. Apply setting plaster to walls and partitions.