Unit 109: Plastering and interior systems

# Worksheet 45: Producing a traditional hard angle (tutor)

1. Arrange these sentences in the correct order of procedures for creating a hard angle using the reverse rule method. Write them in order from 1 to 9.
2. Position rule, ensuring plumb
3. Apply material flush to rule
4. Allow material to set
5. Slide rule away carefully from nib
6. Hold rule to opposite side
7. Check for thickness and plumb
8. Position rule, ensuring plumb
9. Apply material flush with rule to form external angle
10. Slide rule away once material is set and make good