Unit 110: Decorative finishing and industrial painting occupations

# Worksheet 10: Preparation materials (learner)

1. State the two most common abrasive papers used by painters and decorators.
2. What surface defect could be caused if a coarse abrasive paper was used to rub down a smooth surface?
3. Name the type of abrasive paper described below:

*Quicker and more effective than other types of dry abrasives. Does not clog like traditional older abrasive papers, it is sold in 1, 5, 10, and 50 metre rolls*

1. What is the correct name for wet or dry abrasive paper?
2. List five grades of aluminium oxide paper from fine to coarse.
3. List five grades of wet and dry paper from coarse to fine
4. Give an example where you would use the following types of filling material.





............................. .......................... .............................



............................................. .................................................

1. Why is it important not to mix up too much two pack filler?
2. You have been given the task of washing down a factory pre-finished exterior garage door. Write a short sentence on how you would go about the task and what cleaning product you would select.
3. Complete the words using the letters as guidance.

Decorator’s C**.**....... is a F.............. filler ideal for gaps where there is M................ between two S............... It is available in three different colours ....................a ..............n and ...........**...**e It cannot beA..................., so care must be taken not to O**.**....... apply it to a S.................

1. Knotting must be used on knots in timber to:
2. Prevent the sap bleeding through
3. Prevent resin bleeding through
4. Protect the sap from insects
5. Prevent water moisture leaking from the wood
6. Protect the knot from moisture
7. Brushes use in knotting must be washed out using:
8. Surgical spirit
9. Turps
10. Distilled water
11. Fresh water
12. Methylated spirits
13. Which type of filling material would be the ideal choice when filling a gap between two surfaces that are subject to movement?
14. Mark which of the following statements are true or false regarding two pack filler
15. It is soft and very flexible
16. For use on interior and exterior surfaces
17. Some two pack is coloured to match wood
18. It is slow drying
19. Use on wood, metal, and bare plaster
20. What is another name for the hardener used in two pack filler?
21. Complete the missing words in relation to ready-mixed filler.

C....................... wood filler for use before applying V.................

F.......................paste fillers for cracks subject to M....................

AllP................ filler for general small repairs

L.................... filler for general filling but does not dry as hard as other fillers

F................. surface filler for F**.**............ filling