Unit 116: Carry out wall and floor tiling tasks

# Worksheet 41: Wall tiling – applying adhesive (learner)

You should try this task multiple times to allow completion to a satisfactory standard. You should work individually to complete the task. It is advisable to use various sized notch trowels to highlight the different serrating techniques when applying adhesive.

|  |
| --- |
|  |
| **Key points**   * Various dimensions can be used, recommend a minimum of 1m sq. * Learners should practise applying adhesive to a pre-marked out area * Learners to set out area prior to application * Learner has responsibility to ensure backgrounds are suitably prepared * Recommend: use of taping perimeter of practice area * PPE must be worn as appropriate to task * Work area to be kept clean and tidy during activity * Learner to ‘self-score’ and evaluate their work prior to marking by tutor |
| Learners should have overall responsibility for using and maintaining tools and equipment used |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Learner’s name:** |  | **Points (Learning outcome 5.1)** | | | |
| **The learner has:** | **Learning outcome** | **Tutor’s score** | | | **Learner’s self-score** |
| **1** | **2** | **3** |
| *selected and used appropriate tools correctly* | **4.1** | tickbox  Met |  |  |  |
| *suitably prepared background* | **4.2** | tickbox  Met |  |  |  |
| *applied adhesive, even thickness* | **4.5** | tickbox  Met |  |  |  |
| *applied adhesive, serrating lines (same direction)* | **4.5** | tickbox  Met |  |  |  |
| *worn PPE as required with no warnings* | **4.7** | tickbox  ≤ 2 | tickbox  ≥ 1 | tickbox  None |  |
| *kept a clean and tidy work area with no warnings* | **4.7** | tickbox  ≤ 2 | tickbox  ≥ 1 | tickbox  None |  |
| Sub-totals | | /6 | /4 | /6 |  |
| Overall total | | /10 | | | /10 |
| Learner’s evaluation (Learning outcome 5.2) | | | | | |
| Tutor’s comments | | | | | |
| Marked by: …………………………………………. Date completed: ……………………… | | | | | |