Unit 116: Wall and floor tiling

# Worksheet 28: Session summary questions (learner)

1. What is a background?
2. Surface preparation can be defined in **six** key areas. What are they?
3. Which is more rigid, a 12.5 mm or 9.5 mm plasterboard?
4. What is the weight per of a 12.5 mm plasterboard which has been skimmed?
5. What does priming a background do?
6. What is the mix ratio of render?

1. Name **four** cement-based backgrounds.
2. Name **one** advantage of a solid cement-based backer board.
3. When tiling to a timber floor background, what should be installed prior to laying and fixing tiles?
4. Name **one** key process when laying uncoupling membrane on timber.