Unit 202: Changing practices over time

# Worksheet 1: Pre-1919 painting and decorating (Learner)

1. Which film former was the main ingredient of pre-1919 house paints?

|  |
| --- |
|  |
|  |

2. Describe what is meant by limewash. Where it would be used?

|  |
| --- |
|  |
|  |
|  |

3. Traditionally, pre-mixed paints manufactured pre-1919 contained which of the following toxic metals?

a Cobalt.

b Cadmium.

c Lead.

d Aluminium.

4. Which manufacturing process is used to produce anaglypta wallpaper?

|  |
| --- |
|  |
|  |

5. Which wallpaper is described in the following statement?

**‘Deeply embossed wall hanging manufactured from linseed oil putty bonded to a heavy base paper’**

|  |
| --- |
|  |

6. What are the two main methods of printing wallpaper pre-1919?

|  |
| --- |
|  |
|  |

7. Which abrasives were used to prepare surfaces for decoration pre-1919?

|  |
| --- |
|  |
|  |

8. Which filling materials were generally used to make exterior masonry repairs pre-1919?

|  |
| --- |
|  |
|  |

9. Which mineral was the main ingredient used in powder fillers pre-1919?

|  |
| --- |
|  |
|  |

10. State one advantage and one disadvantage of brush application of paints.

|  |
| --- |
|  |
|  |

11. State two adhesives used pre-1919 to hang wallcoverings.

|  |
| --- |
|  |
|  |

12. Describe what is meant by a ‘selvedge’ and state what treatment is required before application.

|  |
| --- |
|  |
|  |
|  |
|  |

13. Traditional limewash/distemper coatings that were used pre-1919 contained which of the following materials?

a Animal fats.

b Charcoal.

c Cement.

d PVA.

14. Which of the following is used as a powdered abrasive?

a Pumice.

b Carbon particles.

c Quartz.

d Silica.