Unit 202: Changing practices over time

# Worksheet 2: Post-1919 construction methods (Tutor)

1. State **two** areas where tiles were produced during this period

Any two of the following:

* Wales
* Manchester
* Dorset

1. How do quarry tiles differ from ceramic tiles?

They are made from quarried materials like clay and shales, fired at a high temperature.

They are stronger than clay tiles.

They are larger and thicker than other ceramic tiles.

1. What was the main difference in fixing techniques for porcelain tiles compared to ceramic tiles?

Unlike ceramic tiles, porcelain tiles did not need to be soaked before fixing, as they have a lower porosity level.

1. What colour was grout during this period?

White or gray.

1. What industry standard for tiling was introduced during this time?

CP202